VIDYASAGAR METROPOLITAN COLLEGE, KOLKATA

Tender No VMC/Office/Building/4/23 dated 22/09/2023

Quotations are invited in sealed cover for the following work from established contractors with proven track record:

1. Dismantling of existing IPS flooring and removal of rubbish
2. Supplying, fitting and fixing and polishing Makrana plain or equivalent grade Marble tile of 15 to 18 mm thickness in floor, over 20 mm (av.) thick base of Cement mortar (1:4) laid with white cement slurry. Area of each slab 2’ x 2.5’ ft (approximately).

Approximate area : 251 sq ft

Time limit of completion of the work 10 days after issue of work order.

Sealed envelope containing quotation, copy of trade license, GST registration certificate and PAN card can be dropped at tender box available near the glass door of new building entrance by 2 p.m of 03/10/2023.

Contact number of the vendor should be clearly mentioned on the outside of the envelope so that vendors can be informed about schedule of opening of tender bids.

Principal