**Common Committee**

Vidyasagar Group of Colleges

39, Sankar Ghosh Lane

Kolkata-700006

**Painting & Repairing of Vidyasagar Statue and Adjacent Area of Vidyasagar Group Of Colleges**

Tender No: VGC/PAINT & REPAIR/2025 -4 Date: 11.01.2025

Quotations are invited in sealed cover for the **Painting & Repairing of Vidyasagar Statue and Adjacent Area of Vidyasagar Group Of Colleges** (old building) 39, Sankar Ghosh Lane Kolkata-700006 as per Annexure from established contractors with proven track record.

**Vendors may visit the actual site during office hours i.e 11 am to 4p.m (Contact :9123318397)**

Time limit of completion of the work **07 days** after issuing of work order.

Interested vendors are requested to submit tender in sealed envelope containing quotation, copy of trade license, GST registration certificate, PAN card and Credentials(if any) *addressing to the* Convener, Common Committee, Vidyasagar Group of Colleges. The Common Committee of Vidyasagar Group of Colleges will not be liable for late receiving of any quotation. The Common Committee of Vidyasagar Group of Colleges has a right to reject any quotation without assigning any reason and the decision will be binding all.

**Important Notes:**

| 1. | Date of Publication of Tender | : | 11.01.2025 |
| --- | --- | --- | --- |
| 2. | Time for Submission | : | 11.00 am to 4.00 pm (except Holidays) |
| 3. | Last date for submission | : | 17.01.2025 upto 2.00pm |
| 4. | Place of Submission | : | Tender box placed at the first floor in front of room no. 9 of Vidyasagar College (old building) 39, Sankar Ghosh Lane Kolkata-700006 |
| 5. | Opening of Tender | : | 17.01.2025 at 2.15 pm |

 Sd/-

 Convener

 Common Committee

Vidyasagar Group of Colleges

**Annexure**

| **Painting & Repairing of Vidyasagar Statue and Adjacent Area of Vidyasagar Group Of Colleges** |
| --- |
|  | **Area of work**  | **Approx Area (sq. Ft)** | **Rate (Rs.)** | **Amount (Rs.)** |
| **Painting****Details of Distemper painting works**Scrubbing of wall.2. Filling the cracks by putty.3. Using distemper paint on wall and ceiling surfaces (2 coats).4. Cleaning of the floors.5. Applying oil enamel paints over scartingPAINTS TO BE USED1. Berger Acrylic DistemperOrAsian Acrylic DistemperOrBirla Acrylic Distemper | Vidyasagar Statue area | 8000 |  |  |
| **Total** |  |

 Sd/-

 Convener

 Common Committee

Vidyasagar Group of Colleges